[InstallShield Silent]
Version=v6.00.000
File=Response File

[File Transfer]
OverwrittenReadOnly=NoToAll

[{94FB906A-CF42-4128-A509-D353026A607E}-DlgOrder]
Dlg0={94FB906A-CF42-4128-A509-D353026A607E}-SdWelcome-0
Count=2
Dlg1={94FB906A-CF42-4128-A509-D353026A607E}-SdFinish-0
Dlg2={94FB906A-CF42-4128-A509-D353026A607E}-RebootDialog-0

[{94FB906A-CF42-4128-A509-D353026A607E}-SdWelcome-0]
Result=1

[Application]
Name=REALTEK Gigabit Ethenet NIC Driver Setup
Version=2.00
Company=REALTEK Semiconductor Corp.
Lang=0009

[{94FB906A-CF42-4128-A509-D353026A607E}-SdFinish-0]
Result=1
bOpt1=0
bOpt2=0

[{94FB906A-CF42-4128-A509-D353026A607E}-RebootDialog-0]
Result=0
Choice=0
